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WELLINGTON FARM HOMEOWNER'S ASSOCIATION
Fence Guidelines
Architectural standards for residential fence installations
1. Approved Materials
	Permitted
	Cedar, pressure-treated wood, redwood, wrought iron, steel, and vinyl.

	Not permitted
	Chain-link fencing is not permitted.

	Plan detail
	Please specify the proposed fence finish on submitted plans.


2. Maximum Fence Height
	72 inches
	Portions of a yard parallel and contiguous to O'Fallon Road or Gutermuth Road.

	72 inches
	Privacy fencing, limited to a total of 40 lineal feet in certain locations immediately behind the home and within all building setback lines.

	48 inches
	All other yard fences.


3. Design Requirements
72-inch fences: May be privacy ("sight-proof") fences.
48-inch fences: Must contain a minimum of 25% open space. For example, 6-inch boards require at least 2 inches of open space between boards. The open area must equal 25% of the total unit (board plus space).
Important: Typical "shadow box" and "board-on-board" designs do not satisfy the 25% open-space requirement.
4. Construction & Approval
• Lot corners should be located by a registered professional land surveyor.
• The fence contractor is responsible for obtaining all applicable permits or variances.
• Trustee approval is required before any fence work begins.
5. Plans & Submission
Please submit an Improvement Submission Form for review before construction begins.
	Before scheduling installation: Confirm that the proposed material, height, design, location, and finish comply with these guidelines and that Trustee approval has been received.
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